Author: ropelt
Company: Schueco International KG

Schüco AWS 65, thermally insulated aluminium window system 
With 65 mm basic depth.

Design features:
Face-fitted vent frame on the room side rebated by 10 mm from the frame edge, flush-fitted on the outside.
The high-volume hollow chamber profile centre gasket is located in the area of the insulation zone.
The system must be fitted with square glazing beads.
The glazing beads are installed with plastic clips to compensate tolerances.

Profile basic depths:
Outer frame, mullion, transom	65 mm
Vent frame	75 mm
Vent frame, flush-fitted	65 mm

Profile face widths:
Outer frame, bottom	104 mm
Outer frame, side and top	79 mm
Mullion	94 mm
Transom	94 mm
Vent frame (window)	41 mm
Vent frame (window door)	61 mm