Last saved by: Hase, Tobias

Schüco ASS 77 PD.HI, insulated Panorama Design system
With continuous 197 mm or 297 mm basic frame depth for maximum transparency and light penetration

Design features:
The modular system consists of 2 different outer frame profiles (90 mm and 150 mm outer frame height). The system is fitted with roller profiles and is thermally broken thanks to PA bars. Furthermore, the system has a drive and locking concept up to safety class 4 that is integrated into the profile and is certified by the TÜV.
The outer frame height adjustment allows you to compensate for building structure tolerances.

Outer frame combination 90/150:
The outer frame combination 90/150 consists of a 90 mm outer frame in the bottom and side section and a 150 mm outer frame in the top section for holding the drive technology. The vents are not visible in this combination (full PD look).

90° corner:
The 90° corner allows for the integration of opening corners and those with fixed glazing.

Outer frame basic depths:
Double-track:	197 mm basic depth
Triple-track:	297 mm basic depth

Face widths:
Outer frame:	0 mm, as it is integrated into the building structure
Vent frame: 0 mm, as it is integrated into the outer frame
Interlock:	37 mm
Double vent:	77 mm

Opening types:
2A, 2A/1, 2B, 2D, 2D/1, 2D 90° corner (inside and outside)
2D/1 90° corner (inside and outside)
3E/1, 3F, 3F 90° corner (inside and outside)

Handles:
Button (provided by customer), DCS integration, integration of smart home BUS system

Vent weights:	Up to 500 kg
Max. vent sizes (W x H):	Up to max. 3200 x 3500 mm
Glass thicknesses:	20 - 60 mm

Test values:
Thermal insulation in accordance with DIN EN ISO 10077-2:	From U_w = 0.96 W/(m²K)*
Wind load resistance in accordance with DIN EN 12210:	Up to class C3/B3
Air permeability in accordance with DIN EN 12207:	Up to class 4
Watertightness in accordance with DIN EN 12208: Up to class 8A
Burglar resistance in accordance with DIN V ENV 1627:	Up to RC2
Operating forces in accordance with DIN EN ISO 13115:	Up to class 1
Resistance to repeated opening and closing in accordance with DIN EN 12400:	Up to class 3
Operating temperature:	-20°C to +50°C
*Calculation basis: Type 2A/1, W x H 5000 x 2700 mm, glass 0.6 W/(m²K), Psi 0.034